****

**ATLAS CSS BOY Operator Interface Requirements Specification**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  |  | | --- | --- | --- | --- | | **APS AES/CTL**  **Specifications Document #** | **ATLAS Operator Interface Requirements Specification** | **Revision** | **0.1** | | **Requirements Specification for ATLAS Operator Interface** | | | |  |  |  |  | | --- | --- | --- | | Alex Dunn |  |  | | Intern, Technical (Author) | Signature | Date | |  |  |  | | Bryan Orr |  |  | | Co-Op, Technical (Author) | Signature | Date | |  |  |  | | Richard Farnsworth |  |  | | Controls Group Leader | Signature | Date | |  |  |  | | Ned Arnold |  |  | | Computer Systems Engineer | Signature | Date | |  |  |  | |  |  |  | |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Version** | **Sections Affected** | **Description of Change** | **Author** | **Date** |
| 00 | All | Initial Document Release | Bryan Orr, Alex Dunn | Jul 23, 2012 |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

CONTENTS

1 INTRODUCTION 5

1.1 Purpose 5

1.2 Scope 5

1.3 Background 5

1.4 References 5

1.5 Assumptions and Constraints 6

1.6 Document Overview 6

2 DESIGN METHODOLOGY 10

3 FUNCTIONAL REQUIREMENTS 10

3.1 User Requirements 10

3.2 Main Power Supply 11

4 OTHER REQUIREMENTS 18

4.1 Hardware Interfaces 18

4.2 Software Interfaces 18

4.3 Communications Interfaces 19

4.4 Hardware/Software Requirements 19

4.5 Operational Requirements 19

4.6 Security 19

4.7 System Reliability 19

4.8 Recoverability 19

4.9 Error Handling 19

5.0 Validation Rules 20

6.0 Conventions/Standards 20

APPENDIX A - GLOSSARY 21

APPENDIX B - Figures 22

APPENDIX C - SCU0 INSTRUMENTATION LIST 25

[Table 1: Summary of functional requirements 6](#_Toc300823206)

[Table 2: Magnet Interlocks 16](#_Toc300823207)

[Table 3: Current Lead Interlocks 16](#_Toc300823208)

[Table 4: SCU0 Warnings Provided 18](#_Toc300823209)

# INTRODUCTION

An operator interface for the Argonne Tandem Linac Accelerator System (ATLAS) utilizing Control System Studio Best Operator Interface Yet (CSS BOY) is required to control and monitor the ATLAS hardware.

## Purpose

This document describes the design requirements of the operator interface for the ATLAS project. The interface is a GUI built on an Eclipse framework called CSS BOY which will interface with EPICS.

## Scope

The interface will be built using CSS BOY from <http://ics-web.sns.ornl.gov/css/products.html> . Although system interfaces are common at Argonne, the use of CSS BOY is new and therefore may require insight into system limitations and deployment structure. Because many of the widgets and display components for ATLAS have already been chosen, the interface will be designed with these specific components in mind.

## Assumptions and Constraints

### Assumptions

Before the operator interface design can begin, the specification requirements document must first be completed and all interested parties must agree to the information contained herein.

Functional testing of the operator interface can be performed using an EPICS soft IOC. Can we access the ATLAS soft IOC?



### Constraints

Time constraints?

## Document Overview

The design methodology will be briefly described before presenting the details of the functional requirements. A section for other requirements will be presented.

The appendices include a glossary of terms used throughout this document as well as interface design diagrams.

Table 1: Summary of functional requirements

# DESIGN METHODOLOGY

# FUNCTIONAL REQUIREMENTS

## User Requirements

There are several different types of users from the standpoint of the control system and they include machine physicists, beamline users, and maintenance personnel. All of these users will generally have the same requirements, differences will be noted.

SCU1.9 Beamline user control shall be in units of energy (eV)

SCU2.0 Machine physicists and SCU0 team shall have control over main coil in (Amps)

SCU2.1 User display shall be either MEDM or CSS BOY to comply with APS standards

## Home Screen Requirements

Highlighted PV’s should be shown on the Home screen. There are more highlighted PV’s than there is space on the home screen.

## Expert Screen Requirements

## Data Buffer Screen Requirements

CSS BOY strip charts.

## Do you not want us to do anything with XGUI?

# OTHER REQUIREMENTS

# Software Interfaces

Currently there is not an interface control document which specifies the software interfaces but for APS all interfaces would be compatible with other APS project applications and would use the EPICS software toolkit which would be developed, deployed, and maintained by the AES Controls Group.

# Communications Interfaces

This control shall be capable of communicating information to and from the system via the LAN using the EPICS Channel Access (CA) communication protocol.

# Hardware/Software Requirements

If a soft IOC were to be used then the system would require an already existing workstation for the IOC to run on; however, if other hardware I/O were to be required then the hardware platform would most likely be the standard APS VME64x rack mounted crate manufactured by Dawn VME Products. The workstation would likely be running Red Hat Linux Enterprise operating system while the VME crate would run the vxWorks operating system; both are compatible with EPICS.

# Operational Requirements

This control system must be operational 24/7 during ATLAS experiments.

# System Reliability

1. A single Eclipse workspace can not be opened in more than one session at a given time. This could pose a challenge if multiple users need to access the interface simultaneously.
2. Magnet quenching which can occur in as little as 10ms could cause stored beam to be inadvertently dumped and should be avoided whenever possible.
3. Since the device is cooled with a closed liquid He system there exists the possibility of the vessel pressure going to a high level which should also be avoided.

# Recoverability

The foreseen failure modes of this system are related to hardware, software, and computer issues; including PV gateway problems. In the event that the system is unavailable to the user due to system failure either hardware or software system recovery must be performed in a timely manner consistent with APS call-in procedures for system recovery and repair.

In the event of a power outage all systems should be powered on with the power supply currents at zero amp output.

A clear role of system component responsibility must be conveyed to those that will be responsible for the equipment required to operate the device.

# Error Handling

Any system errors should be handled automatically by the control system in a failsafe way whenever possible.

# CONVENTIONS AND STANDARDS

All data formats and communication interfaces shall be IEEE compliant.

APPENDIX A - GLOSSARY

CSS BOY – Control System Studio Best Operator Interface Yet

EPICS – Experimental Physics Industrial Control System

GUI – Graphical User Interface

MEDM – Motif Editor Display Manager (Standard APS EPICS Display Screens)

PV – Process Variable (Specific value in EPICS database)

# APPENDIX B - Figures



Figure 1: SCU ID Electrical Connections